**Cấu hình cho Router**

enable

configure

hostname R1

banner motd #R1 duoc cau hinh boi cuongdc#

enable secret 123

line console 0

password 123

login

exit

line vty 0 15

password 123

login

exit

exit

**Cấu hình cho SW1**

enable

configure

hostname SW1

banner motd #cau hinh boi CuongDC HE194183#

enable password 123

line console 0

password 123

login

exit

line vty 0 15

password 123

login

exit

service password-encryption

interface vlan 1

ip address 192.4.8.2 255.255.255.0

no shutdown

ip default-gateway 192.4.8.1

exit

copy running-config startup-config